**Numbered AR tags. All should be 3.54” square. This document in particular is to be used for calibration of the robot using AR tags.**




Figure 1: Marker 8




Figure 2: Marker 7




Figure 3: Marker 6




Figure 4: Marker 5




Figure 5: Marker 4




Figure 6: Marker 3




Figure 7: Marker 2




Figure 8: Marker 1




Figure 9: Marker 0




Figure 10: Marker 9